Note:
Before installing the executive program, proposed closing anti-virus software first strongly! Because in the course of installing, some antivirus software will delete or forbid the materials installed, make the installation fail or cut off.

Version Revision Record
===========================================
V2.6.1 (2023.07.18)
*. Supported Hardware model:
   -Writer: HY10000-WK07x (programming kit)
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P62, HY12P63, HY12P65, HY12P66
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Fixed an abnormal problem caused by insufficient permissions 
    when downloading hex code
===========================================
V2.6 (2018.08.23)
*. Supported Hardware model:
   -Writer: HY10000-WK07x (programming kit)
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P62, HY12P63, HY12P65, HY12P66
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Add in "Chip Code Number".
   -fix the trim range of HAO 4MHz from HY12P62.mem.
===========================================
V2.5 (2017.01.20)
*. Hardware support model:
   -Writer: HY10000-WK07/07B (support OSC Calibration function)
   -Writer: HY10000-WK08C (support OSC Calibration function)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P62, HY12P63, HY12P65, HY12P66
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -Add in "Buzzer function setting".
   -Add in "Checksum function setting".
   -Add in "Writer Version" message window.
   -Add in "Read Burner Setting" function.
   -Add in "Skip frequency trim" function.
   -Documents update
===========================================
V2.40 (2016.08.25)
*. Hardware support model:
   -Writer: HY10000-WK07/07B (support OSC Calibration function)
   -Writer: HY10000-WK08C (support OSC Calibration function)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P62, HY12P63, HY12P65, HY12P66
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32 bit)
   -Windows 7 (64 bit)
   -Windows 8 (32 bit)
   -Windows 8 (64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -Remove function of ID check.
==================================================
V2.30 (2016.03.18)
*. Hardware support model:
   -Writer: HY10000-WK07/07B (support OSC Calibration function)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P62, HY12P63, HY12P65, HY12P66
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32 bit)
   -Windows 7 (64 bit)
   -Windows 8 (32 bit)
   -Windows 8 (64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -Revise the error of "HAO Calibration" at HY12P series.
==================================================
V2.20 (2014.10.07)
*. Hardware support model:
   -Writer: HY10000-WK01, HY10000-WK02, HY10000-WK02B
   -Writer: HY10000-WK05 (support OSC Calibration function)
   -Writer: HY10000-WK06 (support OSC Calibration function)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P63, HY12P65, HY12P66
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32 bit)
   -Windows 7 (64 bit)
   -Windows 8 (32 bit)
   -Windows 8 (64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   Add in -
   -HY12P62
==================================================
V2.10 (2014.04.09)
*. Hardware support model:
   -Writer: HY10000-WK01, HY10000-WK02, HY10000-WK02B
   -Writer: HY10000-WK05 (support OSC Calibration function)
   -Writer: HY10000-WK06 (support OSC Calibration function)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P63, HY12P65, HY12P66
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32 bit)
   -Windows 7 (64 bit)
   -Windows 8 (32 bit)
   -Windows 8 (64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   Add in -
   -Support HID USB communication interface.
==================================================
V2.00 (2013.10.31)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
   -HY12P63, HY12P65, HY12P66
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
   -HY10000-WK06 Writer
*. Add-in support model:
   -HY11P54B
*. Revision items:
   Add in-
   -Add in BIE Read Function at 
	HY11P32, HY11P33, HY11P35, HY11P36,
	HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49,
	HY11P52, HY11P52B, HY11P54, HY11P54B, HY11P58
==================================================
V1.90 (2013.9.2)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P58
   -HY12P63, HY12P65, HY12P66
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
   -HY10000-WK06 Writer
*. Add-in support model:
   -HY12P63, HY12P65, HY12P66
==================================================
V1.80 (2013.7.15)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P54, HY11P58
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
   -HY10000-WK06 Writer
*. Add-in support model:
   -HY11P54, HY11P58
==================================================
V1.70 (2012.12.26)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48, HY11P49
   -HY11P52, HY11P52B, HY11P58
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
*. Add-in support model:
   -HY11P49
==================================================
V1.60 (2012.05.21)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48
   -HY11P52, HY11P52B, HY11P58
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
*. Revision items:
   Revise-
   -Revise the error of "download to flash memory".
==================================================
V1.50 (2012.04.27)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42, HY11P414M, HY11P48
   -HY11P52, HY11P52B, HY11P58
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
*. Add-in support model:
   -HY11P414M
   -HY11P48
   -HY11P58
*. Enhance items:
   -Enhance the software to recognize the chip name function
==================================================
V1.40 (2012.03.12)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42
   -HY11P51, HY11P52, HY11P52B
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
*. Revision items:
   Revise-
   -Revise error in HY11P52B device name.
==================================================
V1.30 (2012.02.24)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42
   -HY11P51, HY11P52
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK02B Writer
   -HY10000-WK05 Writer
*. Add-in support model:
   -HY11P52B
==================================================
V1.20 (2011.12.01)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42
   -HY11P52
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK05 Writer
*. Add-in support model:
   -HY11P51
==================================================
V1.10 (2011.11.22)
*. Support model:
   -HY11P12, HY11P13, HY11P14
   -HY11P22, HY11P23, HY11P24
   -HY11P32, HY11P33, HY11P35, HY11P36
   -HY11P41, HY11P42
   -HY11P52
*. Hardware support model:
   -HY10000-WK01 Writer
   -HY10000-WK02 Writer
   -HY10000-WK05 Writer
*. Program compatibility:
   -Programming file (.HEX) that assembled by HYIDE just can be downloaded form HexLoader Tool.
*. Functional item:
   -Support "Download to flash memory"
   -Support "Read from flash memory"
*. Minimum system requirements for HexLoader programˇG
   -PC compatible PENTIUM system 
   -128MB memory sizeˇ]recommended 256MBˇ^
   -1 GB hard disc space
*. Support operation system: 
   -Windows 98SE 
   -Windows 2000
   -Windows XP
   -Windows Vista
   -Windows 7
   -System support x86,32bit system; not supportive for 64bit system.	
*. Communication interface
   -USB Port